**SEATTLE GALVANIZING COMPANY, INC.**

**General Laborer**

**Nosotros hablamos espanol!**

**If you are a dedicated and punctual individual looking for a fast pace outdoor environment, we would love to hear from you!**

**General Laborer** – Includes work throughout the facility grounds and may include work in areas such as: Wire-up, Cut-down, Clean-up.

Workers must have ability to work in a variety of weather conditions; Must have ability to perform a variety of physical work activities on the job; Must have ability to communicate, understand, and follow directions.

**ESSENTIAL DUTIES/FUNCTIONS INCLUDE BUT ARE NOT LIMITED TO:**

Wire/Chain up steel to racks prior to galvanizing

Un-rack/Cut down steel after being galvanized

Stage materials for flat-bed trucks as necessary

Count, mark, tag parts with customers name and job numbers

Clean galvanized product with files, grinders, wire brushes to remove sharp edges and ridges

Lift product manually or with help of forklifts (Only trained employees operate forklifts)

Identify voids in galvanized coatings and repair using hot sticks, brush or spray on paints, liquid zinc, torches, etc.

Stack materials using pallets and/or dunnage

Shrink wrap and/or band materials

Wear necessary PPE and follow all safety and regulations

Perform cleaning/housekeeping duties as needed

**Salary:**

Once employee transfers over to Seattle Galvanizing payroll:

Pay is $18 an hour for day shift (Mon.-Fri 2:30p-11p occasional mandatory overtime during the week or weekend)

$19 for swing shift (Mon.-Fri 2:30p-11p occasional mandatory overtime during the week or weekend)

**Benefits: (eligible to enroll in benefits after 90 days of employment)**

Medical, Dental, and Vision

Vacation, Sick, and Holiday Pay

Weekly paychecks

Retirement Plan with 3% match

Bonus programs for safety

**Requirements:**

Must be able to perform physical activities that require considerable use of your arms and legs and moving your whole body, such as climbing, lifting, balancing, walking, stooping, and handling of materials up to 75 pounds.

**Work Environment:**

Must be able to work in a wide range of weather conditions in a manufacturing environment under immediate supervision, for long shift periods